**Soil Moisture Sensor Test procedure**

Dummy Load

ADC on Atmega32u4

Micro-Current Sensor

1Meg

200K