Automated Plant Watering Device: Level 1

2.8 V – 4.8 V

Arduino Serial.Println

COM Serial Data –Debug Info

300 mA

8-bit ADC

Moisture Sensor

Open for X seconds – determined by microcontroller

12 V and 5 V

Valve

Power Supply

Power MOSFET

Microcontroller