Automated Plant Watering Device: Level 1

8-bit ADC

Moisture Sensor

Open for X seconds – determined by microcontroller

300 mA

12 V and 5 V

Valve

Power Supply

Power MOSFET

Microcontroller