Water Valve Output: Digital Pin 1

Output High to turn on valve

Moisture Sensor Input: Analog Input 5

Most wet will be high of around 4.3 Volts

Photo Resistor out: Digital Pin 12

Photo Resistor In: Analog Input 4